# Exported Structures and Definitions
[Remote Capture]

## Data Structures
struct | pcap_rmtauth
| This structure keeps the information needed to autheticate the user on a remote machine. More...
struct | pcap_samp
| This structure defines the information related to sampling. More...
## Modules
| Strings related to the new source syntax
| Identifiers related to the new source syntax
| Flags defined in the pcap_open() function
| Sampling methods defined in the pcap_setsampling() function
| Authentication methods supported by the RPCAP protocol
## Defines
#define | PCAP_BUF_SIZE 1024
| Defines the maximum buffer size in which address, port, interface names are kept.
#define | RPCAP_HOSTLIST_SIZE 1024
| Maximum lenght of an host name (needed for the RPCAP active mode).

## Define Documentation

#define PCAP_BUF_SIZE 1024

Defines the maximum buffer size in which address, port, interface names are kept.

In case the adapter name or such is larger than this value, it is truncated. This is not used by the user; however it must be aware that an hostname / interface name longer than this value will be truncated.

Definition at line 79 of file remote-ext.h.

#define RPCAP_HOSTLIST_SIZE 1024

Maximum lenght of an host name (needed for the RPCAP active mode).

Definition at line 399 of file remote-ext.h.

documentation. Copyright (c) 2002-2005 Politecnico di Torino. Copyright (c) 2005-2009 CACE Technologies. All rights reserved.